# Guibo, replace.

Procedure for Guibo is exactly the same as remove and install drive shaft with the exception that you do not remove the rear of the driveshaft.
Remove the Guibo bolts, and the center support bolts and drop the driveshaft in the center, then pull it off the transmission.
Place new Guibo on drive shaft, take note of orientation. There are arrows on the outer edge of the Guibo. These arrows should point towards a flange. |
CAUTION: Do not allow driveshaft to rest on fuel transfer pipe during this procedure.

E30 M3 Repair Manual V2.7. Copyright ©1999-2001 Koala Motorsport & Brett Anderson