# Interior lights, remove and install

Push metal tab in and pull light down. |
Replace bulb. If light assembly is to be replaced, remove wiring. Full time power is supplied via red /green wire from fuse 21. Switched ground from door switches and/or timer control comes via brown / violet wire and full time ground for integral switch via brown wire. |
The interior light is held in place by a plastic frame located above the headliner. It clips into the roof sheet metal. Left side is pictured. |

E30 M3 Repair Manual V2.7. Copyright ©1999-2001 Koala Motorsport & Brett Anderson