# Group 36 Wheel Service bulletins

#### Bulletin number

#### Title

#### Description

#### Date of issue

36 02 84 (893) | Air loss from tires on aluminum wheels | Clean corrosion from rims so that tire seals | January 1985
36 03 84 (938) | Bent alloy rims | Increase in specified tire pressures with load from 26 psi to 29 psi in attempt to prevent rim damage | December 1984
36 04 84 (957) | Wheel centering hub corrosion | Use Plastilube P/N 81 22 9 407 103 to prevent corrosion between wheel and hub | May 1985
36 01 86 (1143) | Snow tire application | Lists appropriate snow tire sizes | September 1988
36 03 86 (1303) | General Tire Information | Warns to use only specified tires on M cars | December 1986
36 01 87 (1377) | Wheel Mounting Procedure | Check to make sure the brake rotor retaining screw is tight and flush or below surface of rotor or wheel bolts could loosen | July 1987
36 02 87 (1390) | Clips for wheel balance weights | Change to single style of clip for two piece wheel weights | October 1987
36 03 87 (1426) | Damage to wheels | Discusses the possibility of wheel damage from driving on a flat. Shows where to check for run-out | July 1987
36 01 88 (1569) | Tire mounting procedure | Do not use Silicone spray to lubricate tire beads when installing | January 1988
36 02 88 (1627) | Balancing of wheel and tire assemblies | Discusses balancing procedure to achieve accurate results | June 1989
36 03 88 (1762) | Paint finish on BMW light alloy wheels | Suggests having wheels bead blasted before repainting to achieve the best results | November 1988
36 02 90 (3150) | Snow tire application chart for 90-91 models | Lists appropriate snow tire sizes | November 1990
36 02 92 (3512) | Wheel fastening bolts | New style has hollow head, is 9 grams lighter than old style, will cause imbalance if mixed | February 1992

E30 M3 Repair Manual V2.7. Copyright ©1999-2001 Koala Motorsport & Brett Anderson