Trim door opening sill plates remove and install

# Door opening sill plates, remove and install.

Use a wide flat object, such as a large screwdriver, under the forward end of the strip to pop the clip out. |
Pull up on the now loose edge of the strip. Use the screwdriver to aid release of other clips if necessary. |
Use pliers to remove clips from floor, replace damaged clips. |

###
Installation:

Install clips in slot on back of sill plate, align clips with holes in floor and gently knock sill plate into position.

E30 M3 Repair Manual V2.7. Copyright ©1999-2001 Koala Motorsport & Brett Anderson