Tail light lense, remove and install

# Tail light lens, remove and install

Remove cover from inside the trunk by turning the two knobs 90°. (88 models on, unscrew single plastic nut in center of cover.) and pulling cover straight into trunk. |
Remove wiring connector from retaining clips holding it in place on the tail light lens. |
Remove the six 8mm nuts from the rear of the lens and slide the lens out of the rear panel. |
Outer 2 nuts retain a bracket that applies clamping force to the side of the tail light opening. |

E30 M3 Repair Manual V2.7. Copyright ©1999-2001 Koala Motorsport & Brett Anderson