Grille for headlights, remove and install

# Grille, headlight section, remove and install

Unlatch hood so that it sits up on its hinge, do not lift hood.

Remove 3 clips from top edge of plastic grille.(green arrows) Remove 2 screws from lower edge, one inboard by kidney grille, the other out under the low beam light.(white arrows) Photo shows kidney grille removed. There is no need to remove kidney grille for this procedure. |

Pull grille straight out and off headlights

E30 M3 Repair Manual V2.7. Copyright ©1999-2001 Koala Motorsport & Brett Anderson