Central locking fuel door actuator

# Central locking fuel door actuator, remove and install

Remove battery cover by twisting 1/4 turn clips 90° and removing. Lift inner edge of cover up, push outer edge down to clear side trunk trim. |
Remove right tail light bulb holder. |
Remove right side trunk trim by pulling the bottom into the trunk. |
Disconnect wiring , remove screws and lift out actuator. |

###
Installation:

"Pistol grip" faces up. |
Place the locking rod (arrow) through the rubber grommet in the body and secure actuator so that the rod will allow the door to open when in the unlocked position. |

E30 M3 Repair Manual V2.7. Copyright ©1999-2001 Koala Motorsport & Brett Anderson