Cylinder head, valve cover, remove and install S14

# Valve cover, remove and install. S14

Remove nuts holding spark plug harness to valve cover, remove spark plug boots and place harness aside. |
Loosen clamp and remove purge hose. |
Remove the eighteen 10mm nuts securing valve cover. |
Remove valve cover. |

###
Installation

Replace gaskets. |

###
Torques :

Valve cover nuts | : | 9 ± 1 Nm (6.5 ± 0.5 ft lbs.)

### Part numbers :

Valve cover gasket - outer | : | 11 12 1 312 171
Valve cover gasket - inner (2 required) | : | 11 12 1 312 173

E30 M3 Repair Manual V2.7. Copyright ©1999-2001 Koala Motorsport & Brett Anderson