Trim front roof liner remove and install

# Front roof liner panel, remove and install.

Use a small screwdriver or similar to pry the lower edge of the check control unit from the roof panel. |
Use a small screwdriver to pry up on connector tab, to release electrical connector from check control unit. |
Open sunroof.
Remove sunroof crank on manual roof models.
Open both front doors and pull down weather stripping on each side in area of liner |
Remove sunvisors. |
Remove visor clips. |
Remove the 7 screws along front edge of sunroof opening and lift off trim strip |
Gently peel back headliner trim and remove two screws under trim strip, one on each front corner of the sunroof opening and remove trim.

E30 M3 Repair Manual V2.7. Copyright ©1999-2001 Koala Motorsport & Brett Anderson