# Air flow meter remove and install

Loosen both 10mm nuts (green arrows), Unplug wiring connector (blue arrow) and loosen clamp (yellow arrow) |
Lift housing up and out of car.
Open air filter housing, remove filter and remove the four 10mm nuts securing air flow meter to air box.

## Installation

Ensure correct positioning of rubber mount at the bottom of the air box assembly.

Replace any seals that show damage.

E30 M3 Repair Manual V2.7. Copyright ©1999-2001 Koala Motorsport & Brett Anderson