Front seats remove and install

# Front seat, remove and install.

Move seats fully rearward, remove caps from nuts and remove the 17mm nut from front of each rail. |
Move seats fully forward and remove the two 17mm bolts from rear of rails. |
Disconnect seatbelt switch wiring from below drivers seat |
Lift seat out of car carefully to avoid damaging paint or trim. |

E30 M3 Repair Manual V2.7. Copyright ©1999-2001 Koala Motorsport & Brett Anderson