# Crash sensor, remove and install.

DANGER: Disconnect battery negative cable before working on SRS system |
Remove the two T30 tamper proof Torx bolts securing crash sensor to inner fender. Disconnect and remove sensor. |

### Installation:

Clean all signs of rust or dirt from the mounting point on the inner fender |
Arrow on sensor faces forward. |

### Torques:

Sensor to inner fender : 8 Nm (6 ft lbs.) |

E30 M3 Repair Manual V2.7. Copyright ©1999-2001 Koala Motorsport & Brett Anderson