Seat belt, rear, remove and install

# Rear seat belt, remove and install.

#### Rear shoulder belt:

Give a sharp upward tug on either side of the front edge of the rear seat's lower cushion. |
Remove single 10mm bolt from each outer corner of the lower backrest. |
Lift backrest upwards to release from brackets on either side of top edge. |
Lift front edge of seatbelt cover on parcel shelf and remove |
Remove 17mm bolts from each rear seatbelt sash. |
Remove speakers.
Unclip panel by lifting up at front edge, and slide tabs out rear bulk head. |
Feed seat belt through parcel shelf trim as you lift it out. |
Remove bolt from inertia reel and remove belt. |

#### Middle belt and all receptacles:

Give a sharp upward tug on either side of the front edge of the rear seat's lower cushion. |
Remove 17mm bolts securing belt to floor. |

### Installation:

Line up inertia reel so that tab is located in slot of reel housing. |

### Torques:

Seatbelts to body : 48 Nm (35 ft lbs.) |

E30 M3 Repair Manual V2.7. Copyright ©1999-2001 Koala Motorsport & Brett Anderson