# Front bumper, Remove and install.

Remove splash shield below engine. |
Disconnect turn signals (green arrows), fog lights (red arrows) and ambient temperature sensor (yellow arrow, left side of car). |  |
Remove 10mm screw (green arrow) and 8mm screw (red arrow) from the splash shield in front of the wheel well. |
Pry out side markers and disconnect wiring. Feed wires back through bumper. |
Pry off bolt covers in bumper cover. |
Remove the 19mm nut below each cover. |
Slide bumper forward to remove, disengaging splash shields as doing so. |

### Installation:

Sides of bumper have brackets that mate with slots on the body. |  |
Slide bumper straight in, checking position of side brackets. |
Push inner fender sections into place behind bumper cover. |

E30 M3 Repair Manual V2.7. Copyright ©1999-2001 Koala Motorsport & Brett Anderson