# Rear side glass remove and install - Opening window.

Remove the side trim panel
Pry plastic cover off rear latch. |
Remove the two Phillips screws securing latch to C pillar. |
Remove Phillips screw from clothes hook on B pillar. Pull clothes hook from B pillar trim. |
Remove 8mm nut from behind coat hook. Use something to stick the nut to the socket or it will drop inside the B pillar. |
Pop off cover from behind seatbelt on B pillar. |
Remove 8mm nut behind cover. Use something to stick the nut to the socket or it will drop inside the B pillar. Slide studs out of B pillar. |
CAUTION: Do not allow glass to fall to the ground.

E30 M3 Repair Manual V2.7. Copyright ©1999-2001 Koala Motorsport & Brett Anderson