Outer window seal, front door, remove and install

# Outer window seal, door, replace.

Lower window. |
Pull plastic cover on inside of door, by mirror, inwards to release. |

####
HiFi System:

Pry door mounted tweeter off door by placing a screw driver approximately 3cm above the tweeter. |
Disconnect wiring and place aside. |

####
All:

Disconnect electrical connector. |
Unscrew two 8 mm retaining bolts, unplug wiring and remove mirror. |
Pull wiring through hole in door and remove mirror. |
Remove sealing strip carefully by lifting up and away from the door. |
Replace any damaged clips. |

### Installation:

Thread wire connector through rectangular hole in door. |
Ensure correct seating of rubber gasket |

E30 M3 Repair Manual V2.7. Copyright ©1999-2001 Koala Motorsport & Brett Anderson