# Oil dipstick tube, remove and install

Remove dipstick |
Disconnect bracket on tube from intake manifold. |
Pull tube straight up while twisting. |

### Installation

Replace seal if fitted, some styles don't use an O ring. |
If no O ring, apply Loctite #270 to the bottom of the tube and drive it in against the stop. |

E30 M3 Repair Manual V2.7. Copyright ©1999-2001 Koala Motorsport & Brett Anderson