# Rear speakers, remove and install

#### Standard system:

Remove screws from speaker cover. |
Lift out speaker and disconnect wiring. |

####
Hi-Fi system :

Gently pry out speaker covers. |
Remove screws from each corner of speaker housing. |
Lift out speaker and disconnect wiring. |

### Installation:

Ensure correct location of speed clips. |
Press covers in starting with edge closest to other cover (Hi Fi system only). |

E30 M3 Repair Manual V2.7. Copyright ©1999-2001 Koala Motorsport & Brett Anderson