# Glove compartment handle, remove and install.

Open glove compartment. |
Remove two Phillips screws from inside of glove compartment door. |
Lift up latch, handle will fall off glove compartment. |
White arrow shows where latch usually breaks. |
After installation , check function of lock. Key vertical (A) is locked Key horizontal (B) is unlocked |

E30 M3 Repair Manual V2.7. Copyright ©1999-2001 Koala Motorsport & Brett Anderson