# Sunroof crank, remove and install

Close sunroof completely. |
Remove screw from cover on crank and remove cover |
Remove screws on either side of crank handle and remove crank. Crank handle must be partially folded before assembly will release from regulator. |
If plastic housing is to be removed, remove screws (arrows) |

### Installation

If crank is installed backwards, handle will not be able to be closed.

E30 M3 Repair Manual V2.7. Copyright ©1999-2001 Koala Motorsport & Brett Anderson