Oil pan baffle, replace

# Oil Pan Baffle, Install.

Remove splash shield from below front of engine. |
Drain engine oil |
Remove the eighteen 10mm lower oil pan bolts |
Remove lower oil pan |
Remove the four 10mm bolts securing the original oil pan baffle (if installed), lift out baffle and install new one. |
Installing a new baffle where one is not currently present requires four 6x10mm bolts. |

### Installation :

Replace pan gasket |

### Torques :

Pan bolts | : | 10 Nm ( 7 ft lbs.) |
Baffle bolts | : | 10 Nm ( 7 ft lbs.) |
Oil drain plug | : | 33 Nm (24 ft lbs.) |

E30 M3 Repair Manual V2.7. Copyright ©1999-2001 Koala Motorsport & Brett Anderson