# Front door, replace

The following procedures should be performed in strict order.

Remove door panel

Remove window

Remove window regulator

Remove mirror

Remove window frame trim

Remove door latch

Remove lock cylinder

Remove exterior door handle

Remove door seal

Remove door stop

Pull wire harness out of door, remove door, transfer weather strip and all clips and clamps to new door and assemble in the reverse of above.

E30 M3 Repair Manual V2.7. Copyright ©1999-2001 Koala Motorsport & Brett Anderson