# Group 72 Equipment & Accessories Service Bulletins

#### Bulletin number

#### Title

#### Description

#### Date of issue

72 01 84 (815) | Roof Racks, 2 door E30 | Seal may remain pushed in after roof rack removal. Push entire length of seal in to achieve good cosmetic appearance | March 1984
72 04 85 (1125) | Front seat belts 9/83 and later | Introduces relocation option of shoulder belt pivot | December 1985
72 01 87 (1325) | Seat /Safety belt components, non interchangeability | Warns of interior swaps causing incompatibility of seat belt components | January 1987
72 03 87 (1541) | Threaded front towing eye 1988 on | Instruction for PDI placement of eye in trunk | January 1988
71 01 88 (1645) | SRS repairs | List of what must be replaced after firing of airbag. | May 1988
72 04 88 (1665) | SRS system component replacement | Request for diagnostic printouts to accompany all SRS parts returns | May 1988
72 01 89 (1789) | SRS Unit Installation Procedure | Describes correct procedure for airbag installation | January 1989
72 03 89 (1835) | Handling of SRS units | Handling and shipping procedures for airbags | March 1989
72 01 90 (3008) | SRS Flash Codes | Lists 2 flash codes omitted from repair manual. | January 1990
72 03 90 (3047) | Seat belt guide, 325i convertible | New guide to prevent belt twisting when allowed to retract rapidly. In production from 3/90 | January 1991
72 02 91 (3338) | SRS diagnostics | Describes how to get fault codes with the BMW service tester. | August 1991
72 04 91 (3388) | Pyrotechnic safety belt tensioner for 92/93 iC | As of 10/91 production, all are fitted with pyrotechnic tensioner | May 1994
72 01 92 (3633) | Testing resistance of airbag igniter circuit | Only Fluke digital volt / ohm meters are approved for this check, use of meters with high testing voltages could ignite airbag | September 1992
72 02 93 (3794) | Collision repair guidelines restraint systems | Must replace airbag, contact ring, impact sensors, control unit and seatbelt tensioner after deployment | May 1994
72 04 93 (3822) | Checking airbag systems | Re-evaluation of 3 yearly inspection requirements. No longer necessary due to self monitoring system | June 1993

E30 M3 Repair Manual V2.7. Copyright ©1999-2001 Koala Motorsport & Brett Anderson