# Fuel gauge , remove and install

Remove instrument cluster

Remove nine gold anodized Phillips head screws from rear of cluster

Squeeze and pull out coding plug

Lift instrument carrier off housing.
Warning : Take extreme care not to damage face of instruments while removing. Place carrier face up in a safe location while it is not being worked on.

Remove nut from rear of fuel gauge and gently pull gauge off circuit board.

### Installation

Align pins of gauge with circuit board and gently press into place.

E30 M3 Repair Manual V2.7. Copyright ©1999-2001 Koala Motorsport & Brett Anderson