SRS control unit

# SRS control unit, remove and install.

DANGER: Disconnect battery negative cable before working on SRS system. |
Remove the four 7 mm hex head screws from bottom edge of trim panel. |
Remove the three Phillips screws securing trim panel to dash. Remove trim panel. |
Pull horizontal panel down and forward. Remove chime module wiring connectors or entire module by spreading the plastic clips securing it to the panel. |
Remove the knee bolster by removing two 10mm bolts on left and three 10mm bolts on right side of bolster. |
WAIT 30 MINUTES! From disconnection of battery, to allow system capacitor to discharge.
Remove the ABS control unit if fitted. 10mm bolts on each side of unit. |
Remove the four 10mm bolts securing the SRS control unit to its mounts.
Remove the ground lead screw from above the control unit and remove the control unit.

### Installation:

Arrows on control unit face forward. |

E30 M3 Repair Manual V2.7. Copyright ©1999-2001 Koala Motorsport & Brett Anderson