# Radio, anti theft, remove and install.

Requires BMW special tool number 82 11 1 466 971 |
Use flat end of tool to open left and right screw covers |
Loosen screws until they stop turning |
Gently grab radio at cassette door and slide out of opening. |
Disconnect wiring from rear of radio. White arrow is wiring, Red arrow is antenna lead. Green arrow shows location of serial number. This serial number is required to obtain the CODE from your dealer. |
C215, pin 1, white, dash lights ; pin 2 , yellow, permanent memory, fuse 21 Cars with ASI radio ( not anti theft ) only have the yellow wire to C215 |

Connectors on rear of anti theft radio.

C216, Pin 1, Violet / Gray, power ; Pin 2, brown/ black, ground

C213, Yellow, left speaker. Contains 2 wires if radio has built in fader.
C214, Blue, right speaker. Contains 2 wires if radio has built in fader.

Single white wire, no connector number, is trigger for power antenna

E30 M3 Repair Manual V2.7. Copyright ©1999-2001 Koala Motorsport & Brett Anderson