Headlight assembly, remove and install

# Headlight assembly, remove and install, non Ellipsoid

Unlatch hood so that it sits up on its hinge, do not lift hood.

Remove 3 clips from top edge of plastic grille.(green arrows) Remove 2 screws from lower edge, one inboard by kidney grille, the other out under the low beam light. (blue arrows) |

Pull grille straight out and off headlights

Remove plastic cover behind headlights by twisting 1/4 turn clips. Unplug headlights |
Remove three screws retaining assembly from front of lights, one on top between the lights, one on the outside of each light. |
Lift out assembly. |

E30 M3 Repair Manual V2.7. Copyright ©1999-2001 Koala Motorsport & Brett Anderson