# Group 63 Lights Service Bulletins

#### Bulletin number

#### Title

#### Description

#### Date of issue

63 01 85 (1014) | Seat belt warning light 85 318i | O2 sensor light discontinued, seat belt light moved to above mirror | April 1985
63 02 85 (1128) | Fog light relay missing E30 prior to 1/1/86 | Install relay during Pre Delivery Inspection | February 1986
63 01 86 (1165) | Fog light wiring connections 325es | Incorrect fog light connector, replace with correct one | February 1986
63 02 87 (1409) | Cleaning of Plastic Parts | Do not use solvents to clean tar or Cosmoline of tail light lenses, lenses will crack. Use fuel oil. | June 1987
63 03 87 (1548) | Headlights / Fog lights remain on when ignition off | Improper relay's, no diodes installed. Replace with diode relays | January 1988
63 01 88 (1601) | Ellipsoid Headlights /Fog lights, condensation | Normal, will dissipate within minutes of light being turned on. Caused by high temperatures and vent system | February 1988
63 02 88 (1732) | Center high mount stop lamp | Warning not to obstruct lamp with stickers or tint | October 1988
63 04 91 (3293) | Interior light delay | New timer, door handle contact eliminated, now uses interior light switch | June 1991

E30 M3 Repair Manual V2.7. Copyright ©1999-2001 Koala Motorsport & Brett Anderson