# Wiper arms, remove and install.

Lift plastic cap at pivot. |
Remove 13mm nut from shaft. |
Raise wiper arm, pull on raised section while lifting with screw driver to rock the arm free of the post. |

### Installation:

Ensure wiper motor is in park position by turning wipers on, then off, and waiting for transmission to stop moving.
Place arms on transmission posts so that blade is level with bottom of windshield, install and tighten nut. |

E30 M3 Repair Manual V2.7. Copyright ©1999-2001 Koala Motorsport & Brett Anderson