# Accelerator pedal lever, remove and install.

#### Non air bag equipped:

Remove three 1/4 turn screws along top edge of panel and one below the steering column |
Pull panel forward and out. Remove chime module from bracket in panel by pulling back tabs. |

#### Air bag equipped:

Remove the four 7 mm hex head screws from bottom edge of trim panel. |
Remove the three Phillips screws securing trim panel to dash. Remove trim panel. |
Pull horizontal panel down and forward. Remove chime module wiring connectors or entire module by spreading the plastic clips securing it to the panel. |
If necessary, remove the knee bolster by removing two 10mm bolts on left and three 10mm bolts on right side of bolster. |

#### All:

Remove accelerator pedal return spring. |
Press off circlip at upper pedal pivot and slide pedal off lever. |
Disconnect throttle cable from lever. |
Remove retainer on lever pivot shaft and slide shaft to the left. |

### Installation:

Lubricate pivot bushings with grease.

E30 M3 Repair Manual V2.7. Copyright ©1999-2001 Koala Motorsport & Brett Anderson