Check control unit, remove and install, 325

# Check control unit, remove and install.

Use a small screwdriver or similar to pry the lower edge of the unit from the roof panel. |
Use a small screwdriver to pry up on connector tab, to release electrical connector from unit. |

Check control unit has 5 bulb holders in the rear, check warnings themselves are non replaceable LEDs.

White arrow : Unit back lighting, with headlights on.
Red arrow : Seat belt warning light
Blue arrow : Not used in US
Green arrow : SRS warning light
Yellow arrow : Not used in US

NOTE: Earlier versions had bulbs staggered but same function in same position. Please contact support@koalamotorsport.com if your country variant uses any of the other bulb positions.

### Installation:

Ensure wiring connector engages correctly. |

E30 M3 Repair Manual V2.7. Copyright ©1999-2001 Koala Motorsport & Brett Anderson