# Group 41 Body Index.

NOTE: Hood, trunk and doors are fitted to an unpainted body shell, adjustment of any of these panels may result in exposure of bare metal. Apply the appropriate color touch up paint to these areas after adjustment has been completed.

Bushings - Door hinge, replace

Bumper - Front, remove and install
Bumper - Rear, remove and install

Front door - Adjust
Front door - Remove and install
Front door - Replace

Hood - Adjust

Trunk lid - Remove and install or adjust

Water leaks - Locations of common leaks.

E30 M3 Repair Manual V2.7. Copyright ©1999-2001 Koala Motorsport & Brett Anderson