# Glove compartment, remove and install.

Open glove compartment and remove pins from restraining straps. |
Press tab on flashlight socket and push socket out of holder. |
Remove wiring clips and remove glove compartment. |
Close glove compartment and loosen the three 10mm nuts along bottom rear edge. Hinge is slotted, allowing it to be removed without totally removing the three nuts. |
Adjust striker after installation. |

E30 M3 Repair Manual V2.7. Copyright ©1999-2001 Koala Motorsport & Brett Anderson