# Window seal, front door, inner, remove and install.

Drivers door: Gently pry out mirror switch and disconnect. |
Passenger door: Pry out plastic cover from armrest. |
Remove screw in opening. |
Remove 2 screws in bottom of armrest. |
Slide armrest forward to disengage clip from storage compartment, remove armrest. Follow green arrows to remove and white arrows to install |
Pry inner door handle surround towards rear of car, and lift off door panel |
If door lock button has a knob on top, unscrew it |
Use a trim tool or gently use a flat screwdriver to pop door panel clips from door, start at the lower front corner where damage will be less noticeable if you make a mistake. |
Once clips are disengaged on bottom and sides of panel, lift panel straight up. Window seal may come out with panel.
If seal does not come out with panel, gently pry upwards on last two clips, grab seal and pull out of remaining clips. |

### Installation:

Align door lock rod with hole in door panel. |
Position window seal on door, not panel, replace any damaged clips. Seal clips go over dimples in sheet metal. |
Replace any damaged door panel or seal clips. |

E30 M3 Repair Manual V2.7. Copyright ©1999-2001 Koala Motorsport & Brett Anderson