# Rear side glass remove and install - Fixed window.

Remove the side trim panel. |
Remove Phillips screw from clothes hook on B pillar. Pull clothes hook from B pillar trim. |
Remove 8mm nut from behind coat hook. Use something to stick the nut to the socket or it will drop inside the B pillar. |
Remove C pillar trim. |
Pull rubber seal down while pushing glass out of frame. |
CAUTION : Do not allow glass to fall to the ground.

E30 M3 Repair Manual V2.7. Copyright ©1999-2001 Koala Motorsport & Brett Anderson