# Slip ring, remove and install

Remove steering wheel

Lift casing off slip ring

Mark position of locking ring to the hub, unscrew the three studs, press the circlip down, turn and remove it.

Lift out the slip ring lock with a screwdriver

Disconnect the plug, remove the three screws in the wheel and remove the slip ring.

### Installation

Mount then new slip ring to the wheel then remove the locking screw visible through the hole between two of the mounting screws.

Place the locking tab spring on the tab and inert the tab into the bore. Press it down until it locks into place.

Place the locking ring on the hub, turn it and pull it up so that the studs appear in the openings.

Lubricate the horn ring with grease.

E30 M3 Repair Manual V2.7. Copyright ©1999-2001 Koala Motorsport & Brett Anderson