# Steering column knuckle, replace.

Remove 13mm nut and bolt from knuckle at rack. |
Remove 13mm nut and bolt from top of knuckle. |
Pry knuckle up on off the rack, then down and off the column. |

### Installation:

Ensure clamp is located on shaft so that bolt hole is lined up with groove in shaft for bolt. |
With steering straight ahead, mark on plastic cap of rack input shaft will line up with cast boss in side of rack. |

### Torques

Knuckle clamps : 22 Nm (15 ft lbs.)
Steering wheel : 80 Nm (58 ft lbs.)

E30 M3 Repair Manual V2.7. Copyright ©1999-2001 Koala Motorsport & Brett Anderson