# Front speakers, remove and install.

### Lower speakers:

#### Left Side, Non air bag equipped:

Remove three 1/4 turn screws along top edge of panel and one below the steering column |
Pull panel forward and out. Remove chime module from bracket in panel by pulling back tabs. |

#### Left Side, Air bag equipped:

Remove the four 7 mm hex head screws from bottom edge of trim panel. |
Remove the three Phillips screws securing trim panel to dash. Remove trim panel. |
Pull horizontal panel down and forward. Remove chime module wiring connectors or entire module by spreading the plastic clips securing it to the panel. |
If necessary, remove the knee bolster by removing two 10mm bolts on left and three 10mm bolts on right side of bolster. |

#### Left side all:

Remove two 8mm screws from release handle. |
Remove screw from lower forward corner of speaker grille. (arrow) |

#### Right Side:

Remove screws from speaker grille. |

#### Both Sides:

Pull edge protector trim away from lower kick panel |
Remove 3 remaining screws from speaker |
Remove speaker and disconnect wiring. 2 wires for standard system, 3 wires for Hi-Fi system |

###
Door mounted tweeters:

Hi-Fi equipped cars have tweeters mounted in the forward corner of the front door window openings.
Pry door mounted tweeter off door by placing a screw driver approximately 3cm above the tweeter. |
Disconnect wiring and place aside. |

E30 M3 Repair Manual V2.7. Copyright ©1999-2001 Koala Motorsport & Brett Anderson