# Rear seat, remove and install.

#### Lower cushion:

Give a sharp upward tug on either side of the front edge of the seat. |

#### Rear cushion:

Remove single 10mm bolt from each outer corner of the lower backrest. |
Lift backrest upwards to release from brackets on either side of top edge. |

### Installation:

Ensure correct seating of backrest on brackets. |
Lock seat belts in their holders if equipped, or place on top of seat cushion. Push rear edge of seat cushion in as far as possible, then push front edge down so that clips engage seat. |
Seat base has openings for metal clips mounted to floor (above). |

E30 M3 Repair Manual V2.7. Copyright ©1999-2001 Koala Motorsport & Brett Anderson