# Group 32 Steering & Wheel Alignment Service Bulletins

#### Bulletin number

#### Title

#### Description

#### Date of issue

32 01 83 (766) | Noise in steering column and wheel, 318i | Steering column touches surround, place washer P/N 17 11 9 932 650 between the collar and wheel | September 1983
32 02 84 (834) | Steering wheel lock E30 | Remove lock and housing and check tumblers for free movement, replace lock or housing depending on results | September 1984
32 03 84 (848) | Front Axle Camber Adjustment | Eccentric upper strut mounts are available for adjustment | July 1984
32 04 84 (868) | Replacement of steering gear due to accident | Discusses when to replace steering gear after an accident | September 1984
32 06 84 (891) | Power steering gear for handicapped persons | Up to 40% more assist, LHD P/N 32 13 1 128 422 RHD P/N 32 13 1 129 277 | April 1985
32 02 85 (1061) | Power steering system noises at low temperatures | Replace ATF with LHM fluid P/N 81 22 9 407 025 | July 1985
32 04 85 (1098) | Key blanks from HUF will not fit ignitions | Grind stop shoulder on code side of key | October 1985
32 01 86 (1186) | Engine noises in passenger compartment | Plug missing form end of hollow steering shaft, remove emblem from wheel and plug column with DUM-DUM | March 1986
32 02 86 (1281) | Recall Campaign 86V-138 ; steering coupling | Install plates on column knuckle to prevent it separating , causing loss of steering in accident | December 1986
32 01 87 (1433) | Steering lock assembly production change | Shows change to pin hole for release of lock cylinder | July 1987
32 02 88 (1594) | M Technik sport steering wheel | Horns do not work or run continuously, deformed horn contacts, replace with new P/N 32 33 1 155 956 | February 1988
32 05 88 (1763) | Steering column universal joints | Do not allow high pressure water or steam to strike the universals to prevent grease being washed out. | November 1988
32 03 89 (1880) | Power steering cooler pipe 325iX | If cooler is present, remove and replace existing hoses with P/N 32 41 1 137 750. Cooler can cause pressure build up that may rupture the line from rack to cooler | September 1989
32 03 91 (3320) | Power steering noise except iX | From 6/90 to 10/91 may have a pressure hose with spiral coil. Replace with hose without coil M20 P/N 32 41 137 153, M42 P/N 32 41 1 133 399 | November 1991

E30 M3 Repair Manual V2.7. Copyright ©1999-2001 Koala Motorsport & Brett Anderson