Side markers

# Side markers, front and rear, remove and install.

Orange side markers are for front use only, red for rear use only.
One end of the light has a small slot in it. Insert the tip of a screwdriver in this slot and gently pry out. When edge of light is out of bumper cover, slide light out. |
Disconnect socket by turning ¼ turn. Bulb pulls straight out of socket. |

### Installation:

These lights are known to crack along the top of the bulb area, this allows water to enter the light, corroding the bulb holder and wiring connector. Before installation of the light, smear some black or clear silicone sealer over the cracked area. |

### Part Numbers:

Front side marker, Orange | : | 63 14 1 385 419
Rear side marker, Red | : | 63 14 1 385 420
Bulb | : | 07 11 9 978 373

E30 M3 Repair Manual V2.7. Copyright ©1999-2001 Koala Motorsport & Brett Anderson