Emblem, model designation, replace

# Emblem, model designation, replacing.

Model designation emblems are secured with double sided tape.
Cut old emblem off by sawing with a lubricated piece of string or fishing line.
Clean residual glue from trunk lid.
Install new emblem using the following measurements for correct location.
Emblem base is to be 19mm from lower edge of trunk lid Measure 75mm in from right side of trunk to left side of figure 3. Measure 9mm from left side of figure 3, to right side of letter M |

E30 M3 Repair Manual V2.7. Copyright ©1999-2001 Koala Motorsport & Brett Anderson