Trim parcel shelf remove and install

# Parcel shelf trim, remove and install.

Give a sharp upward tug on either side of the front edge of the rear seat's lower cushion. |
Remove single 10mm bolt from each outer corner of the lower backrest. |
Lift backrest upwards to release from brackets on either side of top edge. |
Lift front edge of seatbelt cover on parcel shelf and remove |
Remove 17mm bolts from each rear seatbelt sash. |
Remove speakers.
Unclip panel by lifting up at front edge, and slide tabs out rear bulk head. |
Feed seat belt through parcel shelf trim as you lift it out. |

### Installation:

Speaker openings are marked on rear of trim panel in cars without rear speakers. |
Ensure correct seating of backrest on brackets. |
Lock seat belts in their holders if equipped, or place on top of seat cushion. Push rear edge of seat cushion in as far as possible, then push front edge down so that clips engage seat. |
Seat base has openings for metal clips mounted to floor (above). |

E30 M3 Repair Manual V2.7. Copyright ©1999-2001 Koala Motorsport & Brett Anderson