# Trunk trim panels remove and install

ALL : Remove floor mat

### Seatback panel

Remove 4 expanding rivets across panel and remove panel

### Left side panel

Remove jack

Remove rear trim panel, see below

Pull trim down from top, then lift out. Take car with jack holder.

### Right side panel

Remove battery cover, if applicable

Remove seatback panel, see above

Remove rear panel, see below

Lift panel out from the bottom

### Rear panel

Push down pins in upper trim until they fall through.

Remove clips and take off upper trim

Remove tail light covers by twisting both 1/4 turn clips, or unscrewing the single knob on later cars.

Pull out rear panel from bottom.

E30 M3 Repair Manual V2.7. Copyright ©1999-2001 Koala Motorsport & Brett Anderson