# Multi-Function clock, remove and install

Using a small screw driver or pick, pull face plate from unit. |
Squeeze tabs at top and bottom of unit and pull out of housing. Lift up on black lever beside wiring connector do disconnect unit. |
Change display illumination bulb (red arrow) and button back lighting bulb (green arrow). |

### Installation

Ensure wiring connector is fully seated and lever is locked down. |
Push unit into dash until tabs lock into place, refit face plate. |

E30 M3 Repair Manual V2.7. Copyright ©1999-2001 Koala Motorsport & Brett Anderson