# Group 16 Fuel Supply Service Bulletins

#### Bulletin number

#### Title

#### Description

#### Date of issue

16 01 84 (864) | Use of oxygenated fuels | Use in pre 84 models will void warranty, all other models will not suffer damage if oxygenated fuels are used. | July 1984
16 02 84 (937) | Imported US models with catalytic converter | Euro delivery cars run on leaded fuel require catalytic converter and O2 sensor replaced and fuel system flushed. Not covered by warranty. | March 1985
16 01 86 (1199) | Hard or no start, noisy fuel pump. Pre delivery pump not working correctly | Pre pump dead, or feed hose split. | August 1986

E30 M3 Repair Manual V2.7. Copyright ©1999-2001 Koala Motorsport & Brett Anderson