# Window 2 door rear side glass replace

Remove side window

Remove trim and rubber seal from old window

Install new seal new window.

Install trim by starting at upper edge of window and working around. Use a silicone fluid to aid assembly

If the window has been broken, remove rear seat back and clean glass from seatbelt reels.

E30 M3 Repair Manual V2.7. Copyright ©1999-2001 Koala Motorsport & Brett Anderson