# Adjust clutch pedal

To adjust the pedal, the pivot bolt between pedal and clutch master cylinder push rod is eccentric.

Turn the eccentric pivot so that the dot on the head is facing away from the master cylinder.

The eccentric can only be positioned in one of two positions, 180° apart, due to the nature of forces exerted on the pivot point, if it is not in one of the two positions, it can slip, causing loss of adjustment.

E30 M3 Repair Manual V2.7. Copyright ©1999-2001 Koala Motorsport & Brett Anderson