# Alternator, diode plate, replace

Disassemble alternator
De-solder stator coil on diode plate.
CAUTION: Use a low heat setting, excess heat from a soldering iron can damage diodes.
Remove six screws located around perimeter of diode plate, remove the plate.
Check condition of insulating sleeves and washers on wiring posts before installation of a new diode plate.

E30 M3 Repair Manual V2.7. Copyright ©1999-2001 Koala Motorsport & Brett Anderson