# Headlights, aim.

Check and correct tire pressure

Fill fuel tank and place approximately 70 kg, 155 lbs., in the rear seat.

Check aim of lights.

If adjustment is required, open hood and remove covers behind each set of lights. |
Adjustment is achieved via white knobs. Red arrows for horizontal adjustment Green arrows for vertical adjustment Picture shows right headlights, left light in picture is high beam, right light is low beam. |

E30 M3 Repair Manual V2.7. Copyright ©1999-2001 Koala Motorsport & Brett Anderson